{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["大会堂"],"read":"whole","date_system":"1900"}

{"sheet":"大会堂","index":0,"n_rows":169,"n_cols":10,"rows_kept":169,"merged":[[0,0,0,9],[92,0,92,7],[92,8,92,9],[102,0,108,0],[102,1,108,1],[102,8,108,8],[102,9,108,9],[109,0,115,0],[109,1,115,1],[109,8,115,8],[109,9,115,9],[116,0,122,0],[116,1,122,1],[116,8,122,8],[116,9,122,9]]}
["党校-大会堂舞台设备"]
["序号","名称","技术参数","单位","数量","规格型号","推荐品牌","原产地","单价","合计"]
["一、","大会堂舞台机械设施设备"]
["1.1、","吊杆系统"]
["1.1.1","前檐幕吊杆","吊点数：5吊点，行程：18m，速度：0～0.6m/s（变频调速），载荷：6.0kN（活载荷），定位精度：±3mm，运行噪音：≤48dB","道",1,"进口电机、电器，国内加工","定制"]
["1.1.2","大幕机","对开行程：13m，对开速度：0～1.0m/s（变频调速，均匀收缩），载荷：8.0kN（活载荷），定位精度：±3mm，运行噪音：≤45dB","套",1,"进口电机、电器，国内加工","定制"]
["1.1.3","电动吊杆","吊点数：5吊点，行程：18m，速度：0～0.6m/s（变频调速），载荷：6.0kN（活载荷），定位精度：±3mm，运行噪音：≤48dB","道",12,"进口电机、电器，国内加工","定制"]
["1.1.4","灯光吊杆","吊点数：5吊点，行程：18m，速度：0～0.3m/s（变频调速），载荷：10.0kN（活载荷），定位精度：±3mm，运行噪音：≤48dB","道",7,"进口电机、电器，国内加工","定制"]
["1.1.5","二幕机","吊点数：5吊点，对开行程：13m，对开速度：0～1.0m/s（变频调速），载荷：2.5kN（活载荷），定位精度：±3mm，运行噪音：≤45dB","套",1,"进口电机、电器，国内加工","定制"]
["1.1.6","侧光吊杆","吊点数：4吊点，行程：18m，平移方式：手动，升降速度：0～0.3m/s（变频调速），载荷：10.0kN（活载荷），定位精度：±3mm，运行噪音：≤48dB","套",2,"进口电机、电器，国内加工","定制"]
["1.1.7","柱光架","尺寸：宽1.5m×高8.5m×厚0.8m.四排挂灯杆，可上人操作调整灯具","套",2,"现场加工","定制"]
["1.1.8","天幕框","尺寸：宽16m×高8.5m金属框架","套",1,"现场加工","定制"]
["1.1.9","PLC变频控制系统","电动吊杆、灯光吊杆、大幕机、二幕机均由PLC控制系统集中控制","套",1,"进口原件，现场编程","定制"]
[null,"吊杆系统小计"]
["2、","幕布系统"]
["1.2.1","沿幕：","麻绒,高3米×宽18米×3倍褶","付",1,null,"定制"]
["1.2.2","大幕：","麻绒，高9米×宽22米×3倍褶","付",1,null,"定制"]
["1.2.3","二道幕：","麻绒，高9米×宽22米×3倍褶","付",1,null,"定制"]
["1.2.4","横幕","麻绒,高3米×宽18米×3倍褶","付",4,null,"定制"]
["1.2.5","侧幕：","麻绒，高9米×宽3米×3倍褶","付",8,null,"定制"]
["1.2.6","底幕","白色细帆布，高10米×宽20米×1倍褶","付",1,null,"定制"]
[null,"幕布系统小计"]
[null,"机械幕布系统总计"]
["二、","大会堂音响扩声系统"]
["序号","名称","技术参数","单位","数量","规格型号","推荐品牌","原产地"]
[2.1,"调音控制网络及路由系统"]
["2.1.1","主控数字调音台","80路混音输入\n64路话筒单声道输入\n4路立体声输入和4路专用FX返送，可外加8路可分配外置插入\n24编组/辅助/FX输出\n所有编组都有8个矩阵输出和发送，辅助，FX和左、中、右主线\n12个VCA编组和8个独立哑音编组\n每条输入、输出通道都有4组全参数均冲器\n每条输入带有高通滤波器\n35组30段BSS技术的图示均冲器\n每条输入通道带压缩器、噪声门`、每条输出通道带压缩器\n4个独立的立体声莱思康效果的FX处理器","台",1,"Soundcraft  VI3000","Soundcraft/MIDAS/DIGICO","原装进口"]
["2.1.2","网络输出接口卡","64入64出","台",1,"Soundcraft  RN344","ROCKNET /Soundcraft/MIDAS","原装进口"]
["2.1.3","备用数字调音台","48路话筒单声道输入\n4路立体声输入和4路专用FX返送，可外加8路可分配外置插入\n24编组/辅助/FX输出\n所有编组都有8个矩阵输出和发送，辅助，FX和左、中、右主线\n12个VCA编组和8个独立哑音编组\n每条输入、输出通道都有4组全参数均冲器\n每条输入带有高通滤波器\n35组30段BSS技术的图示均冲器\n每条输入通道带压缩器、噪声门`、每条输出通道带压缩器\n4个独立的立体声莱思康效果的FX处理器","台",1,"Soundcraft  VI3000","Soundcraft/MIDAS/DIGICO","原装进口"]
["2.1.4","主备调音台同步器","满足主备调音台实时数据同步","台",1,null,"Soundcraft/MIDAS/DIGICO","原装进口"]
["2.1.5","远程网络接口箱","16个MIC/Line输入接口和8个输出接口","台",3,"RN.101.IO","ROCKNET /Soundcraft/MIDAS","原装进口"]
["2.1.6","远程网络接口箱","8个数字输出接口","台",2,"RN.332.DO","ROCKNET /Soundcraft/MIDAS","原装进口"]
["2.1.7","MADI输出卡",null,"块",2,"SIO-C5D","Rocknet/VENUE/HDSPe","原装进口"]
["2.1.8","跳线盘","48口跳线盘，根据各自系统设计,可调整连接逻辑方式\n每台跳线盘配置1/6跳线口数量跳线，规格按需","台",8,"SWITCHCRAFT MT48FN","Neutrik/SWITCHCRAFT/HIROSYS","原装进口"]
["2.1.9","无源音频分配器","12通道话筒输入，三组12通道（36路）输出\n工作电平可达+26dBu\n拥有PPD幻像电源直通专利技术","台",4,"PLS MS08","HIROSYS/XTA/SWITCHCRAFT","原装进口"]
["2.1.10","监听耳机","能量转换器：动圈、封闭；\n频率范围：≥20-20kHz；","副",2,"Audio-Technica  ATH-M50","Audio-Technica/SHURE/Sennheiser","原装进口"]
["2.1.11","监听音箱","2 路低音反射式双功放近场工作室监听音箱，配备6.5“ 锥形低音单元和 1” 半球形高音单元。\n43Hz - 30kHz 频率响应。\n60W LF 以及 35W HF 双功放系统，高性能 95W 功率放大能力","台",2,"YAMAHA HS7","YAMAHA/JBL/真力","原装进口"]
["2.1.12","网络交换机","企业级、千兆24口","台",2,"CISICO",null,"原装进口"]
[2.2,"音乐播放系统"]
["2.2.1","数字音频工作战","24英寸商用办公一体机电脑\n i5 2G独显，8G内存，1T硬盘","台",1,"联想扬天S800","联想/IBN/DELL","原装进口"]
["2.2.2","专业外置声卡","12输入和12输出通道外置USB声卡 \n4 x 模拟输入(话筒、线路、乐器)\n1 x MIDI I/O\nADAT I/O或1 x SPDIF I/O光","台",1,"RME Babyface Pro","Roland/YAMAHA/RME","原装进口"]
["2.2.3","专业CD播放机",null,"台",1,"DENON DN-C635","TASCAM/DENON/Fostex","原装进口"]
["2.2.4","数字固态录音、播放机",null,"台",1,"DENON DN-F450R","TASCAM/DENON/Fostex","原装进口"]
["2.2.5","播放控制键盘",null,"台",1,"DENON RC-F400S","TASCAM/DENON/Fostex","原装进口"]
[2.3,"扬声器系统"]
["2.3.1","中央声道全频线阵列扬声器组","2分频，线阵列全频扬声器\n频响范围(±3 dB)：60 Hz - 18 kHz\n指向性(-6 dB) H x V：110° x 10°\n最大声压级（SPL）：141.3 dB\n阻抗： LF 8Ω HF 8Ω\n功率 (AES / Peak)：LF 2x 350 / 2x 1400 W\n                   HF 160 / 640 W","只",8,"ADAMSON S10-i","ADAMSON/MeyerSound/NEXT","原装进口"]
["2.3.2","左声道全频扬声器组","2分频，线阵列全频扬声器\n频响范围(±3 dB)：60 Hz - 18 kHz\n指向性(-6 dB) H x V：110° x 10°\n最大声压级（SPL）：141.3 dB\n阻抗： LF 8Ω HF 8Ω\n功率 (AES / Peak)：LF 2x 350 / 2x 1400 W\n                   HF 160 / 640 W","只",8,"ADAMSON S10-i","ADAMSON/MeyerSound/NEXT","原装进口"]
["2.3.3","右声道全频扬声器组","2分频，线阵列全频扬声器\n频响范围(±3 dB)：60 Hz - 18 kHz\n指向性(-6 dB) H x V：110° x 10°\n最大声压级（SPL）：141.3 dB\n阻抗： LF 8Ω HF 8Ω\n功率 (AES / Peak)：LF 2x 350 / 2x 1400 W\nHF 160 / 640 W","只",8,"ADAMSON S10-i","ADAMSON/MeyerSound/NEXT","原装进口"]
["2.3.4","低音扬声器","低音扬声器\n频响范围(±3 dB)：30 Hz - 80 Hz\n最大声压级（SPL）：138 dB\n阻抗：8Ω\n功率 (AES / Peak)：1200 / 4800 W","只",4,"ADAMSON S119-i","ADAMSON/MeyerSound/NEXT","原装进口"]
["2.3.5","下拉声像扬声器","频率范围：55Hz-18KHz；\n最大声压级（连续／峰值）：136dB\n角度（垂直*水平）：40°x 20° / 60°x 40°；\nLF（ND15L）：15’’ ,8欧；HF（B&C DE800）：1.4’’, 16欧；\n额定阻抗：8欧\n功率(AES/峰值）：LF：500W/2000W；HF：110W／440W；","只",4,"ADAMSON  Point 15-p","ADAMSON/MeyerSound/NEXT","原装进口"]
["2.3.6","台唇补声扬声器"," 频率范围：72Hz-18KHz；\n 最大声压级：128dB；\n 角度（垂直*水平）：70°x 70°\n 阻抗内置分频：4Ω\n 灵敏度：MF：91dB；HF：107.5dB；\n 尺寸：32.1 cmx17.1cm x 17.2cm","只",7,"ADAMSON  Point Concentric 5","ADAMSON/MeyerSound/NEXT","原装进口"]
["2.3.7","楼座补声扬声器","频率范围：60Hz-18KHz；\n最大声压级：134.4dB；\n角度（垂直*水平）：40°x 20° /60°x40°\nLF（ND12）：12’’，8欧；\nHF（B&C DE800）：1.4’’，16欧；\n额定功率(AES/峰值）：610W/2440W","只",6,"ADAMSON  Point 12-p","ADAMSON/MeyerSound/NEXT","原装进口"]
["2.3.8","固定返听扬声器","频率范围：55Hz-18KHz；\n最大声压级（连续／峰值）：136dB\n角度（垂直*水平）：40°x 20° / 60°x 40°；\nLF（ND15L）：15’’ ,8欧；HF（B&C DE800）：1.4’’, 16欧；\n额定阻抗：8欧\n功率(AES/峰值）：LF：500W/2000W；HF：110W／440W；","只",4,"ADAMSON  Point 15-p","ADAMSON/MeyerSound/NEXT","原装进口"]
["2.3.9","流动返听扬声器","频率范围：50Hz-18KHz\n最大声压级：137.8dB(外分频)；137.3dB（内分频）\n角度（垂直*水平）：50°x 50° \n阻抗/单元尺寸LF（ND15）：15’’ ,8欧；HF（B&C DE1000）：1.5’’, 8欧\n功率(AES／峰值）：LF：500W／2000W；HF：140W／560W","只",4,"ADAMSON  M15","ADAMSON/MeyerSound/NEXT","原装进口"]
["2.3.10","环绕声扬声器","12寸同轴扬声器\n频率范围：64Hz-18KHz；\n最大声压级：133dB；\n角度（垂直*水平）：60°x 40°\n功率(AES/节目源／峰值）：MF：350W／700W/1400W；HF: 80W／160W/320W\n额定功率(AES/峰值）：430W/1720W\n灵敏度：MF：95dB；HF：104.7dB；","只",28,"  Point Concentric 12","ADAMSON/MeyerSound/NEXT","加拿大"]
["2.3.11","线阵扬声器吊装件",null,"套",3,"S-Series Support Frame","ADAMSON/MeyerSound/NEXT","原装进口"]
["2.3.12","补声扬声器吊装件",null,"套",38,null,null,"定制"]
["2.3.13","主扩声系统功放","4通道功放，带4通道处理器\n最大输出功率：(all channels driven)\n4 ohms：3000 W","台",5,"PLM+ 12k44 /SP ","CAMCO/LAB/REYN-AUDIO","原装进口"]
["2.3.14","后场补声扬声器功放","2通道功放，带2通道处理器\n最大输出电压（per channel）：70 Vrms\n最大输出电流（per channel）：20 Arms\n最大输出功率：(all channels driven)\n4 ohms：1200 W","台",1,"PLM+ 12k44 /SP ","CAMCO/LAB/REYN-AUDIO","原装进口"]
["2.3.15","返听功放","内部处理能力 32bit\n采样率 44.1kHz 48kHz 88.2kHz 96kHz\n64四通道音频处理能力\n具备GPI、RS232C/RS422、USB和 MIDI 等多种外部控制接口","台",2,"PLM+ 12k44 /SP ","CAMCO/LAB/REYN-AUDIO","原装进口"]
["2.3.16","环绕及台唇补声功放","内部处理能力 32bit\n采样率 44.1kHz 48kHz 88.2kHz 96kHz\n64四通道音频处理能力\n具备GPI、RS232C/RS423、USB和 MIDI 等多种外部控制接口","台",9," IPD 2400 ","CAMCO/LAB/REYN-AUDIO","原装进口"]
[2.4,"无线话筒"]
["2.4.1","双通道无线话筒接收机","无线射频频率范围： 516.....865 MHz\n载波频率个数：3000 \n预设个数：64 \n交换频宽： 75 MHz 峰值频偏：+/- 48 kHz \n静噪阀值： Off, 5 ... 25 dBμV   \n互调间距： ≥ 75 dB  \n天线插座： 2 BNC (50 OHM)Product  \n可堆叠插座： 2 BNC (50 OHM)   \n增益： 0 dB ±0,5 dB  \n降噪器： HDX \n频率响应范围： 25 ... 18000 Hz   \n信噪比： > 120 dB(A)   THD, \n总谐波失真： < 0,9 %","台",6,"sennheiser EM 2000-CW ","Sennheiser/SHURE/AKG","原装进口"]
["2.4.2","手持发射机连动圈话筒头","UHF手持式发射机,动圈话筒头","套",4,"sennheiser SKM 2000BK-CW/MMD945","Sennheiser/SHURE/AKG","原装进口"]
["2.4.3","腰包发射机","尺寸极小，高切换带宽\n与无线话筒接收机配套\n可切换输出功率","台",8,"Sennheiser SK 2000-CW","Sennheiser/SHURE/AKG","原装进口"]
["2.4.4","微型领夹话筒头","全方向形微型领夹话筒，含配套夹子","个",8,"Sennheiser MKE2-4","Sennheiser/SHURE/AKG","原装进口"]
["2.4.5","微型耳挂话筒头","头戴式电容话筒，黑色，全方向形","个",8,"Sennheiser HSP2","Sennheiser/SHURE/AKG","原装进口"]
["2.4.6","放大天线","与无线话筒配套使用","套",2,"Sennheiser AD3700","Sennheiser/SHURE/AKG","原装进口"]
[2.5,"有线话筒"]
["2.5.1","鼓套装话筒","1×大鼓话筒+4×军鼓话筒+2×乐器话筒","支",1,"sennheiser E 600 SERIES DRUM SET","Sennheiser/SHURE/AKG","原装进口"]
["2.5.2","心形动圈话筒","指向特征心型\n收音头动圈式\n灵敏度2 mV/Pa±3dB\n频率范围40-18000Hz\n产品声压350dB","支",4,"sennheiser E 935","Sennheiser/SHURE/AKG","原装进口"]
["2.5.3","超心形动圈话筒","指向特征超心型\n收音头动圈式\n灵敏度2 mV/Pa±3dB\n频率范围40-18000Hz\n产品阻抗350欧姆 ","支",4,"sennheiser E 945","Sennheiser/SHURE/AKG","原装进口"]
["2.5.4","小振膜电容录音话筒","指向特性：心型\n频率范围：20 Hz - 20 kHz\n灵敏度，额定值为1 kHz时±2 dB：10 mV/Pa; -40 dB re. 1 V/Pa\n等效噪音电平，A加权：Typ. 20 dB(A) re. 20 μPa (max. 23 dB(A))\nS/N比（A加权）, re. 1 kHz @ 1 Pa (94 dB SPL)：Typ. 74 dB(A)\n动态范围：Typ. 117 dB\n削波前最大声压级：153 dB\n衰减器开关：0 dB / -20 dB","支",12,"DPA 2011","Sennheiser/DPA/AKG","原装进口"]
["2.5.5","大振膜合唱话筒","频率响应20-20,000 Hz\n高通滤波80 Hz, 12 dB/octave\n开路灵敏度-32 dB (25.1 mV) re 1V at 1 Pa\n阻抗100 ohms\n最大输入声压级145dB SPL(1KHz,THD 1%)\n噪声12 dB SPL\n动态范围 (典型值)133 dB, 1 kHz at Max SPL\n信噪比82 dB, 1 kHz at 1 Pa","支",5,"Audio-Technica AT4040  ","Sennheiser/SHURE/Audio-Technica","原装进口"]
["2.5.6","立体声DI盒","DI盒，乐队乐器专用转换盒；","台",4,"APEX dBDI-2","APEX/K.T/XTA","原装进口"]
["2.5.7","话筒立杆",null,"只",20,"K&M   ","K&M /TAKASAGO/Audio-Technica","原装进口"]
["2.5.8","数字会议发言主机","可以为多达50台会议话筒底座供电\n通过多台控制机组串联连接后，最高可操作多达150台会议话筒底座\n设有4组可作配置的平衡式音频输出，以及1组与输出1相同的非平衡输出\n设有2组话筒/线路输入，以及2路辅助(AUX)输入和2组返回输入\n除了当前的语言外，2组返回输入可作为其他2种语言的同声传译配置\n会议模式：自由发言、请求发言、远程控制\n覆盖模式：无覆盖、后进先出(LIFO)、先进先出(FIFO)\n触发话筒：手动按键 或 语音激活",null,null,"Audio-Technica  ATUC-50CU","Audio-Technica/VEENO/RH","原装进口"]
["2.5.9","数字会议发言单元","可作独立编程的多样配置及多种用途底座装置 ： 主席或代表\n与标准的3针XLR卡农话筒兼容的鹅颈话筒连接插座\n话筒前置放大器采用低噪声（EIN ： 127分贝）的分立式晶体管，并设有个别（每席发言装置）的可调增益控制\n配备了高音质及能增强语音清晰度的扬声器\n24bit/48 kHz的数字音频质量",null,null,"Audio-Technica ATUC-50DU","Audio-Technica/VEENO/RH","原装进口"]
["2.5.10","数字会议专用鹅颈话筒","背极电容式\n超心形指向\n频率响应100～15,000Hz\n灵敏度-40dB (10.0 mV) 以 1V 于 1 Pa\n最大输入声压级134dB S.P.L. / 1 kHz 于 1% T.H.D.\n信噪比64dB以上 / 1 kHz 于 1 Pa\n阻抗250Ω，平衡",null,null,"Audio-Technica  ATUC-M43H","Audio-Technica/VEENO/RH","原装进口"]
[2.6,"工程辅材"]
["2.6.1","UPS 不间断电源","3KVA/0.5H","台",1,"伊顿 9130-9130i 3000R-XL2U","EATON/Santak/EATON","中国"]
["2.6.2","机柜","19\"42U 800mm加深型","台",3,"图腾 42U","图腾/金盾/爽通","中国"]
["2.6.3","时序电源","16A,8口,带滤波功能","套",3,"国产优质","国产优质","中国"]
["2.6.4","音频接插件","选用进口品牌，满足系统安装工艺需求","批",1,"NEUTRIK","Neutrik/SWITCHCRAFT/HIROSYS","原装进口"]
["2.6.5","超五类网线","满足系统安装工艺需求","批",1,"AMP或以上品牌","成丰/华敏/森格","中国"]
["2.6.6","音频信号线","满足系统安装工艺需求","批",1,"成丰","成丰/华敏/森格","中国"]
["2.6.7","扬声器信号线","满足系统安装工艺需求","批",1,"成丰","成丰/华敏/森格","中国"]
["2.6.8","天线馈线","阻抗50欧，满足系统安装工艺需求","批",1,"国产优质","成丰/华敏/森格","中国"]
["2.6.9","镀锌管线、桥架 ","满足系统安装工艺需求；符合国标、项目标准线管、桥架、防火","批",1,"国产优质","国产优质","中国"]
["2.6.10","接口箱/盒","满足系统安装工艺需求","套",2,"国产优质","国产优质","中国"]
["2.6.11","舞台地盒面板","满足系统安装工艺需求","套",4,"国产优质","国产优质","中国"]
["2.6.12","其它安装附材及安装配件","根据系统需求定制","批",1,"国产优质","国产优质","中国"]
["音响设备总计"]
["三、","大会堂舞台灯光系统"]
["序号","名称","技术参数","单位","数量","规格型号","推荐品牌","原产地"]
[3.1,"灯光控制系统"]
["3.1.1","综合调光控制台(主)","6个标准DMX 512信号输出口\n内置8,192 HTP/LTP-控制\n参数可通过网络扩展\n30个电动程序执行推杆\n5个转轮\n1个轨迹球\n3个内置触摸屏。\n2个外置SVGA显示器接口\n2个以太网端口\n2个USB接口","台",1,"彩熠 TEKMAND III","YEL/MA2/FINE ART","中国"]
["3.1.2","综合调光控制台(备)","6个标准DMX 512信号输出口\n内置4,096 HTP/LTP-控制参数\n可通过网络扩展\n15个电动程序执行推杆\n5个转轮\n1个轨迹球\n2个内置触摸屏。\n2个外置SVGA显示器接口\n2个以太网端口\n2个USB接口","台",1,"彩熠 TEKMAND II","YEL/MA2/FINE ART","中国"]
["3.1.3","电脑（含灯光控制软件）","含键盘、鼠标、22寸显示器\n含WYSINYG及同档次灯光控制软件\nCPU不低于Intel 至强E3-1200 v3\n内存不小于4G\n硬盘容量不小于1TB\n光驱:DVD-ROM","台",1,"联想 ThinkServer RS240 ","联想/IBN/DELL","中国"]
["3.1.4","便携式笔记本","I5及以上CPU\n屏幕尺寸不小于14英寸\n内存不小于4G\n硬盘不小于500G\nDVD刻录","台",1,"联想 ideapad 510S","联想/IBM/DELL","中国"]
["3.1.5","控制室应急电源","备用UPS电源(2KW/0.5H)机架式","套",1,"伊顿 9130-9130i 3000R-XL2U","EATON/Santak/EATON","中国"]
["3.2","灯光信号传输系统"]
["3.2.1","灯光信号网络中继柜（控制室）","三层24口网络交换机(含光纤接口、满足双光纤环绕)\n支持POE供电模式\n不少于24个10/100Mbps接口，不少于2个SFP千兆位以太网端口\n传输速率不小于10M/100Mbps\n支持SNMP和WEB管理功能","台",1,"S5700-24TP-SI-AC ","HUAWEI/CISCO/H3C ","中国"]
[null,null,"配线架24口","台",1,"AMPCOM 19\"24","优质国产","中国"]
[null,null,"以太网转DMX信号分配器(2048)","台",1,"ON001R(8CH)","COMPULITE/ETC/HIGH END/MA","中国"]
[null,null,"DMX跳线盘","台",4,null,"优质国产","中国"]
[null,null,"DMX信号放大器1进8出","台",4,"EXPLODER(12CH)","优质国产","中国"]
[null,null,"备用UPS电源(2KW/0.5H)机架式","台",1,"9130-9130i 3000R-XL2U","优质国产","中国"]
[null,null,"19寸标准机柜含相关辅材配件","台",1,"19”42u","图腾/金盾/爽通","中国"]
["3.2.2","灯光信号网络中继柜（调光柜）","三层48口网络交换机(含光纤接口、满足双光纤环绕)\n支持POE供电模式\n不少于48个10/100Mbps接口，不少于4个SFP千兆位以太网端口\n传输速率不小于10M/100Mbps\n支持SNMP和WEB管理功能","台",1,"S5700-48TP-SI-AC 48","HUAWEI/CISCO/H3C ","中国"]
[null,null,"配线架48口","台",1,"AMPCOM 19\"48","优质国产","中国"]
[null,null,"以太网转DMX信号分配器(2048)","台",1,"ON001R(8CH)","COMPULITE/ETC/HIGH END/MA","中国"]
[null,null,"DMX跳线盘","台",8,null,"优质国产","中国"]
[null,null,"DMX信号放大器1进8出","台",8,"EXPLODER(12CH)","优质国产","中国"]
[null,null,"备用UPS电源(2KW/0.5H)机架式","台",1,"9130-9130i 3000R-XL2U","优质国产","中国"]
[null,null,"19寸标准机柜含相关辅材配件","台",1,"19”42u","图腾/金盾/爽通","中国"]
["3.2.3","灯光信号网络中继柜（栅顶）","三层24口网络交换机(含光纤接口、满足双光纤环绕)\n支持POE供电模式\n不少于24个10/100Mbps接口，不少于2个SFP千兆位以太网端口\n传输速率不小于10M/100Mbps\n支持SNMP和WEB管理功能","台",1,"S5700-24TP-SI-AC ","HUAWEI/CISCO/H3C ","中国"]
[null,null,"配线架24口","台",1,"AMPCOM 19\"24","优质国产","中国"]
[null,null,"以太网转DMX信号分配器(2048)","台",2,"ON001R(8CH)","COMPULITE/ETC/HIGH END/MA","中国"]
[null,null,"DMX跳线盘","台",6,null,"优质国产","中国"]
[null,null,"DMX信号放大器1进8出","台",6,"EXPLODER(12CH)","优质国产","中国"]
[null,null,"备用UPS电源(2KW/0.5H)机架式","台",1,"9130-9130i 3000R-XL2U","优质国产","中国"]
[null,null,"19寸标准机柜含相关辅材配件","台",1,"19”42u","图腾/金盾/爽通","中国"]
["3.2.4","流动E/D盒","以太网转DMX信号分配器(1024)","台",4,null,"优质国产","中国"]
["3.2.5","场灯/工作灯控制系统","36路3KW场灯/工作灯控制系统\n4分控点控制面板","套",1,"HDL-MDH1210/MPL8","ADB/ STRAND/HDL","中国"]
[3.3,"调光柜"]
["3.3.1","调光立柜","96路，具有状态报告功能，符合一级标准。","台",3,"D96","ADB/ STRAND/HDL","中国"]
["3.3.2","调光模块","调光模块，3KW/回路，具有实时报告回路亮度、电流等参数功能,高效抑制电感器，上升时间大于200us。","路",192,"调光模块","ADB/ STRAND/HDL","中国"]
["3.3.3","继电器模块","继电器模块，3KW/回路，具有实时报告回路亮度、电流等参数功能","路",96,"开关模块","ADB/ STRAND/HDL","中国"]
[3.4,"灯具"]
["3.4.1","5°高效成像聚光灯","600W-1000W，符合CE标准或UL标准；显色指数Ra>92；色温3200K；光束角度：5度，含灯勾、灯泡、保险链、360°旋转灯架、色片夹和灯尾线","盏",24,"PH750-5","德晟 /PHIDA/MONON","中国"]
["3.4.2","10°高效成像聚光灯","600W-1000W，符合CE标准或UL标准；显色指数Ra>92；色温3200K；光束角度：10度，含灯勾、灯泡、保险链、360°旋转灯架、色片夹和灯尾线","盏",24,"PH750-10","德晟 /PHIDA/MONON","中国"]
["3.4.3","19°高效成像聚光灯","600W-1000W，符合CE标准或UL标准；显色指数Ra>92；色温3200K；光束角度：19度，含灯勾、灯泡、保险链、360°旋转灯架、色片夹和灯尾线","盏",24,"PH750-19","德晟 /PHIDA/MONON","中国"]
["3.4.4","大功率LED变焦聚光灯","功率300W；灯珠3W*108pcs（28R+28G+28B+24W);角度7°-50°；尺寸：253*250mm;防护IP20","盏",72,"PS-3108Z4","德晟 /PHIDA/MONON","中国"]
["3.4.5","LED变焦聚光灯","功率185W；灯珠3W*61pcs（15R+14G+14B+18W);角度7°-50°；尺寸：253*232.5mm;防护IP65","盏",160,"PS-361Z4","德晟 /PHIDA/MONON","中国"]
["3.4.6","LED投光灯","额定功率不小于560Wmax；\nLED灯珠不少于188颗；红绿蓝白琥珀5种颜色混合；\n控制方式：DMX512、声控、自动、主从\n不少于8标准控制通道\n调光：0-100%；\n频闪：0-20HZ；\n光学角度45x60°\n含灯钩、保险链","组",24,"WS-3942","德晟 /PHIDA/MONON","中国"]
["3.4.7","全功能光束电脑灯","光源规格：TI_SIRIUS HRI 440W；平行光束角度0°~2°可调；线性调光：机械线性调光0~100%；频闪速度每秒1-20次 \n；1个固定颜色轮有14个色片+白光，可半色效果、线性色彩转换及双向变速旋转彩虹效果；1个旋转图案轮有12个可选图案片+白光，可变速抖动/双向流动；2个独立旋转棱镜，棱镜互相组合生成奇特多光束效果；1个独立的雾化效果，光斑柔和自然","盏",36,"GTD-440 II/ I BSW","德晟 /PHIDA/MONON","中国"]
["3.4.8","追光灯","2.5KW 氙气灯泡；含整流器、灯架、灯泡","盏",2,"PH2500","德晟 /PHIDA/MONON","中国"]
["3.4.9","三基色会议灯","4*55W","盏",30,"4*55","德晟 /PHIDA/MONON","中国"]
["3.4.10","低烟机","功率不小于3000W，标准DMX512及线控、无线遥控，油桶容量不小于6升，温机时间不大于12分钟，直接热保护装置，烟量输出40,000 cu.ft/min，最大耗油量5 min/Liter，配带轮航空箱","台",2,"W530","安特利 ","中国"]
["3.4.11","泡泡机","功率：200W，线控及无线遥控，容量1.5升，最大耗油量50ml/min，配带轮航空箱","台",2,"B200","安特利","中国"]
["4.5","线缆桥架及辅材"]
["3.5.1","舞台灯光阻燃电缆","3*4mm²；（阻燃、低烟、无卤）","米",30000,"WDZN-RYJY-3*4mm²","金博","中国"]
["3.5.2","以太网控制信号线缆","超五类线","米",3000,null,"专业定制","中国"]
["3.5.3","DMX信号线缆","RVVP2*0.35","米",5000,null,"专业定制","中国"]
["3.5.4","光纤线缆","多模光纤","批",1000,null,null,"中国"]
["3.5.5","金属桥架各类弯通","根据实际需求定制","批",1,null,"国标材料","中国"]
["3.5.6","钢管","根据实际需求定制","批",1,null,"国标材料","中国"]
["3.5.7","网络接插件-插座（固定式）","网络接口/卡侬型","批",1,null,"国标材料","中国"]
["3.5.8","DMX接插件-插座（固定式）","DMX512接口","批",1,null,"国标材料","中国"]
["3.5.9","电源转接箱","16A欧标防水插","批",1,null,"国标材料","中国"]
["3.5.10","各类工程辅料","满足使用要求","批",1,null,"国标材料","中国"]
[null,"小计"]
["4、","大会堂大屏幕显示系统"]
["序号","名称","技术参数","单位","数量","规格型号","推荐品牌","原产地"]
[4.1,"舞台背景大屏"]
["4.1.1","舞台背景P4 LED全彩显示屏","点距P4mm；有效显示面积24米宽，8米高、独立金属箱体、含钢构","㎡",192,null,"利雅得/迈锐/祎鑫","中国"]
["4.1.2","信号发送接收系统",null,"项",1,null,"诺瓦、","中国"]
["4.1.3","播控主机","i7、独显","台",1,null,"国产优质","中国"]
["4.1.4","视频处理器","DVI、HDMI、VGA、AV多格式多节目源无缝互切","台",1,null,"国产优质","中国"]
["4.1.5","电源管理系统",null,"套",1,"ABB","ABB","中国"]
[4.2,"台口两次大屏"]
["4.2.1","舞台背景P2.5高清LED全彩显示屏","点距P2.5mm；有效显示面积4米宽，3米高、独立金属箱体、含钢构；两块","㎡",24,null,"利雅得/迈锐/祎鑫","中国"]
["4.2.2","信号发送接收系统",null,"项",1,null,"诺瓦、","中国"]
["4.2.3","播控主机","i7、独显","台",1,null,"国产优质","中国"]
["4.2.4","视频处理器","DVI、HDMI、VGA、AV多格式多节目源无缝互切","台",1,null,"国产优质","中国"]
["4.2.5","电源管理系统",null,"套",2,"ABB","ABB","中国"]
[null,"小计"]
[null,"大会堂系统总计",{"$nulls":7},{"v":28000000,"d":"28000000.00"}]