{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["礼堂音响灯光"],"not_rendered":{"images":6},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"礼堂音响灯光","index":0,"n_rows":8,"n_cols":10,"rows_kept":8,"merged":[[0,0,0,5],[0,6,0,9],[2,0,2,9],[7,1,7,7]],"flags":["formulas_cached_only"]}
["演出音响方案"]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价","小计","类似图"]
["一、扩声系统"]
[1,"双10寸线阵音箱","Wharfedale","WLA-210","WLA-210线阵列音箱是一个中型两路驱动的两分频音箱。提供50Hz-16KHz的频率范围。两个44mm(音圈)的钕磁压缩高音单元，两个10寸钕磁低音单元构成一个动态余量极大的组合。\n\nWLA-210的中低频部分使用一对400W的10寸纸盆低音单元，两只低音串联工作。高频部分使用两只44mm(音圈)钕磁压缩单元,通过一个平面波转换器结合一个90度的指数曲线恒指向号筒,产生一个一致的波阵面。高达112dB灵敏度的高频部分,使WLA-210产生高达138db的峰值声压输出。\n\nWLA-210的箱体为梯形,箱体与箱体之间的间隙已经缩到最小.每只箱体的可调角度为0-10度,每1度可调. 吊挂件使用高强度钢材制成，在吊挂16只音箱时，吊挂件具备7：1的安全系数。箱体由面板18mm,其他15mm的夹板构成，表面为耐磨的黑色点纹油漆。2个与箱体平齐内嵌的把手安装在音箱两侧，方便搬运。黑色的穿孔铁网保护音箱单元。\n\n主要特点：\n\n \n\n◆HiFi级的听感，浑厚有弹性的低频，清亮通透的高频\n\n◆可预置度的吊挂件\n\n \n规格参数\n频率响应：70Hz-16KHz（±3dB），60Hz-18KHz（-10dB）\n指向性（H×V）：90°×10°\n灵敏度(2.83V/1m)：HF：111dB SPL，LF：100dB SPL\n功率：持续LF：800W，HF：80W；节目：LF：1600W，HF：160W；峰值：LF：3200W，HF：320W\n最大声压级（@1m）：HF：136dB；LF：135dB\n额定阻抗：HF：16Ω；LF：16Ω\n低音单元：2×10\"（3\"音圈）钕铁硼\n高音单元：1×3\"（1.4\"出口）钕磁压缩式高音\n连接器：2×NL4\n角度：0-10°可调\n尺寸(H×W×D)：303×730×509mm\n净重：32kg\n","只",12]
[2,"双15寸线阵低音音箱","Wharfedale","WLA-215B","类型：双15寸次低频音箱\n频率响应：38Hz-200Hz（±3dB），25Hz-320Hz（-10dB）\n灵敏度(2.83/1V)：102dB\n功率：1200W\n最大声压级：133dB SPL,139dB SPL peak\n阻抗：8Ω\n低音单元：2×15\"（3\"音圈）铁氧体\n连接器：2×NL4\n尺寸(H×W×D)：605×730×700mm\n净重：65kg","只",4]
[3,"线阵主音4*1400W功放","COBRA-2","Vortex 1400QD+","1400Wx4/8Ω，2300Wx4/4Ω\n频率响应：20Hz-20kHz(+0/-1.5dB)\n总谐波失真：≤0.05％\n信噪比：≥95dB\n阻尼系数：≥800\n输入灵敏度：0.775V/1.0V/1.4V/38dB/32dB/26dB\n输入阻抗（平衡/不平衡）：20kΩ/10kΩ\n电压增益（8Ω时）：40.3dB\n冷却:从前到后抽风","台","3"]
[4,"低音2*2050W功放","COBRA-2","Vortex 2050D+","2050Wx2/8Ω，3550Wx2/4Ω\n频率响应：20Hz-20kHz(+0/-1.5dB)\n总谐波失真：≤0.05％\n信噪比：≥95dB\n阻尼系数：≥800\n输入灵敏度：0.775V/1.0V/1.4V/38dB/32dB/26dB\n输入阻抗（平衡/不平衡）：20kΩ/10kΩ\n电压增益（8Ω时）：40.3dB\n冷却:从前到后抽风","台","2"]
[5,"合计",{"$nulls":6},584562,"以上报价不含税不含运费不含安装调试费税费另加10%"]