{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":5},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":10,"rows_kept":7,"merged":[[0,0,0,5],[0,6,0,9],[2,0,2,9],[6,1,6,7]]}
[]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价","小计","类似图"]
[]
[1,"一拖一无线手持话筒","SHURE","SLX24/SM58","SM58话筒配备SLX2手持式发射机：\n• 发射机类型：手持式\n• 音频输入电平：位于-10dB位置时较大值为+2 dBV，位于0dB位置时较大值为-8 dBV\n• 增益调整范围：10dB\n• 射频发射机输出：较大值为30 mW（视各国适用的规定而定）\n• 外壳：模塑PC/ABS把手和电池盖\n• 电源：2节AA碱性电池或充电电池\n• 电池，供电时间：2节AA电池，> 8小时\n• 尺寸（包含SM58拾音头）：254 x 51mm\n• 重量： 290g（10.2盎司），不含电池\nSLX4 分集接收机：\n• 电源：PS21\n• Battery Status：是\n• 外壳：镀锌钢\n• 音频输出电平：XLR接口（连接至600 Ω负载）：-13 dBV 1/4英寸接口（连接至3000 Ω负载）：–2 dBV\n• 输出阻抗：XLR接口： 200 Ω，1/4英寸接口： 1 kΩ\n• 灵敏度：-105 dBm，12 dB信噪比（典型值）\n• 镜频抑制：>70 dB（典型值）\n• 典型条件下的工作范围：100米（300英尺）\n• 音频频率响应：（+/-2 dB）：最小： 45 Hz，较大：15 kHz\n• 尺寸：高42 x 宽197 x 深134（mm）\n• 重量：816g","套",4]
[2,"天线分配器","COEFMIC","WA-ATKS","低噪放大电路设计. \n八通道低损耗天线分配电路设计,4套单频道自动选讯接收机可共同一对天线. \nBNC接头,保证连接可靠性. \n技术参数:\n天线输入阻抗/Antenna Input Impedance:50 ohms \n天线输出阻抗/Antenna Ouput Impedance:50 ohms \n天线;输入插座/Antenna Input Receptacle:BNC \n天线输出插座/Antenna Output Receptacle:BNC \n增益/Gain:3dB \n带宽/Bandwidth:450-950MHz \n供电/Power Requirements:DC12-18V 2000mA \n尺寸/Dimensions:45*410*160mm \n重量/Weight:200g","台",1]
[3,"定向宽频天线","COEFMIC","WA-KS","单一方向接收天线,能有效减少其他设备对接收机的干扰。\n高增益设计，能有效增加接收距离。 \n技术参数:\n频率范围/Resonate Frequency Range:450~900MHz \n驻波比/Standing Wave Ratio:<1.3 \n增益/Gain:7dBi \n尺寸/Dimensions:279*267mm \n重量/Weight:180g","只",2]
[4,"合计",{"$nulls":6},{"$f":"17180*2","v":34360}]